{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["cenik2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":32,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"cenik2","index":0,"n_rows":128,"n_cols":10,"rows_kept":128,"cut":false,"hidden":false,"merged":[[120,0,120,9],[106,0,106,9],[0,1,0,4],[0,6,0,9],[1,2,2,2],[1,6,2,6],[1,3,2,3],[1,4,2,4],[63,0,63,9],[1,7,2,7],[1,1,2,1],[1,8,2,8],[47,0,47,9],[20,0,20,9],[3,0,3,9],[1,9,2,9],[0,0,2,0]],"flags":["formulas_cached_only"]}
["název zboží         aktualizováno 3.3.2004","cena  bez DPH",{"$nulls":4},"cena s DPH "]
[null,"měrná     jednotka","za měrnou jednotku","balení","za jedno  balení",null,"měrná     jednotka","za měrnou jednotku","balení","za jedno  balení"]
[]
["ZDÍCÍ MATERIÁLY"]
["CIHLA PLNÁ pálená P20","ks",5.5,"1 ks",5.5,null,"ks",6.71,"1 ks",6.71]
["CIHLA PLNÁ pálená P30","ks",5.95,"1 ks",5.95,null,"ks",7.259,"1 ks",7.259]
["CIHLA LEHČENÁ","ks",5.5,"1 ks",5.5,null,"ks",6.71,"1 ks",6.71]
["CIHLA CDM 24","ks",5.55,"1 ks",5.55,null,"ks",6.771,"1 ks",6.771]
["CIHLA DUTÁ 2děr.","ks",4.5,"1 ks",4.5,null,"ks",5.49,"1 ks",5.49]
["CIHLA DUTÁ 4cm (vanovka)","ks",13,"1 ks",13,null,"ks",15.86,"1 ks",15.86]
["CIHLA VP BÍLÁ 24","ks",6.3,"1 ks",6.3,null,"ks",7.686,"1 ks",7.686]
["CIHLA VP BÍLÁ 29","ks",6.9,"1 ks",6.9,null,"ks",8.418000000000001,"1 ks",8.418000000000001]
["CIHLA BETON.29","ks",10,"1 ks",10,null,"ks",12.2,"1 ks",12.2]
["CIHLA ŠAMOTOVÁ 25","ks",25.5,"1 ks",25.5,null,"ks",31.11,"1 ks",31.11]
["CIHLA ŠAMOTOVÁ 30","ks",29.5,"1 ks",29.5,null,"ks",35.99,"1 ks",35.99]
["TVÁRNICE šedá 40x30x25","ks",40,"1 ks",40,null,"ks",48.8,"1 ks",48.8]
["HURDIS 100","ks",48,"1 ks",48,null,"ks",58.56,"1 ks",58.56]
["HURDIS 110","ks",48,"1 ks",48,null,"ks",58.56,"1 ks",58.56]
["HURDIS 120","ks",48,"1 ks",48,null,"ks",58.56,"1 ks",58.56]
["HURDIS PATKA","ks",5.9,"1 ks",5.9,null,"ks",7.198,"1 ks",7.198]
["SUPERTHERM"]
["SUPERTHERM 49 P+D P10 490/247/238","ks",54.9,"1 ks",54.9,null,"ks",66.978,"1 ks",66.978]
["SUPERTH.  49 P+D P10 1/2 490/125/238","ks",28.7,"1 ks",28.7,null,"ks",35.013999999999996,"1 ks",35.013999999999996]
["SUPERTHERM 44 P+D P10 440/247/238","ks",49.3,"1 ks",49.3,null,"ks",60.145999999999994,"1 ks",60.145999999999994]
["SUPERTHERM 44 P+D P15 440/247/238","ks",52.8,"1 ks",52.8,null,"ks",64.416,"1 ks",64.416]
["SUPERTH.  44 P+D P10 1/2 440/125/238","ks",25.8,"1 ks",25.8,null,"ks",31.476,"1 ks",31.476]
["SUPERTHERM 40 P+D P10 400/247/238","ks",43.1,"1 ks",43.1,null,"ks",52.582,"1 ks",52.582]
["SUPERTHERM 40 P+D P15 400/247/238","ks",45.9,"1 ks",45.9,null,"ks",55.998,"1 ks",55.998]
["SUPERTHERM 40 R      P10 400/147/238","ks",26.9,"1 ks",26.9,null,"ks",32.818,"1 ks",32.818]
["SUPERTH.  40 P+D P10 1/2 400/125/238","ks",22.5,"1 ks",22.5,null,"ks",27.45,"1 ks",27.45]
["SUPERTHERM 36,5 P+D P10 365/247/238","ks",37.2,"1 ks",37.2,null,"ks",45.384,"1 ks",45.384]
["SUPERTHERM 36,5 P+D P15 365/247/238","ks",42.4,"1 ks",42.4,null,"ks",51.727999999999994,"1 ks",51.727999999999994]
["SUPERTH.  36,5 P+D P10 1/2 365/125/238","ks",19.4,"1 ks",19.4,null,"ks",23.668,"1 ks",23.668]
["SUPERTHERM 30 P+D P10 300/247/238","ks",28.6,"1 ks",28.6,null,"ks",34.892,"1 ks",34.892]
["SUPERTHERM 30 P+D P15 300/247/238","ks",29.6,"1 ks",29.6,null,"ks",36.112,"1 ks",36.112]
["SUPERTHERM 30 R      P10 300/147/238","ks",22.9,"1 ks",22.9,null,"ks",27.938,"1 ks",27.938]
["SUPERTH.  30 P+D P10 1/2 300/125/238","ks",15.5,"1 ks",15.5,null,"ks",18.91,"1 ks",18.91]
["SUPERTHERM 24 P+D P10 240/372/238","ks",35,"1 ks",35,null,"ks",42.699999999999996,"1 ks",42.699999999999996]
["SUPERTHERM 24 P+D P15 240/372/238","ks",35.7,"1 ks",35.7,null,"ks",43.554,"1 ks",43.554]
["SUPERTH. 19/Týn P+D P10 190/497/238","ks",44.2,"1 ks",44.2,null,"ks",53.924,"1 ks",53.924]
["SUPERTHERM 17,5 P+D P10 175/497/238","ks",40.5,"1 ks",40.5,null,"ks",49.41,"1 ks",49.41]
["SUPERTHERM 17,5 P+D P10 175/372/238","ks",28,"1 ks",28,null,"ks",34.16,"1 ks",34.16]
["SUPERTHERM 11,5 P+D P10 115/497/238","ks",31.2,"1 ks",31.2,null,"ks",38.064,"1 ks",38.064]
["SUPERTHERM 11,5 P+D P10 115/372/238","ks",21.5,"1 ks",21.5,null,"ks",26.23,"1 ks",26.23]
["SUPERTHERM  14 P+D  P10 140/497/238","ks",37.5,"1 ks",37.5,null,"ks",45.75,"1 ks",45.75]
["SUPERTHERM 6,5 P+D P15 65/333/238","ks",15,"1 ks",15,null,"ks",18.3,"1 ks",18.3]
["KERAMICKÉ PŘEKLADY SUPERTHERM ","ks",null,"1 ks",null,null,"ks",null,"1 ks"]
["CIHLA  POROTHERM"]
["POROTHERM 44  P+D  P-8","ks",52.6,"1 ks",52.6,null,"ks",64.172,"1 ks",64.172]
["POROTHERM 44  P+D  P-10","ks",54,"1 ks",54,null,"ks",65.88,"1 ks",65.88]
["POROTHERM 44  P+D  1/2 P-10,15","ks",28.2,"1 ks",28.2,null,"ks",34.403999999999996,"1 ks",34.403999999999996]
["POROTHERM 40  P+D  P-8","ks",45.8,"1 ks",45.8,null,"ks",55.876,"1 ks",55.876]
["POROTHERM 40  P+D  P-10","ks",47.2,"1 ks",47.2,null,"ks",57.584,"1 ks",57.584]
["POROTHERM 40  P+D  1/2 P-10,15","ks",24.6,"1 ks",24.6,null,"ks",30.012,"1 ks",30.012]
["POROTHERM 36,5  P+D  P-8","ks",39.8,"1 ks",39.8,null,"ks",48.556,"1 ks",48.556]
["POROTHERM 36,5  P+D  P-10","ks",40.7,"1 ks",40.7,null,"ks",49.654,"1 ks",49.654]
["POROTHERM 36,5  P+D  1/2 P-10,15","ks",21.2,"1 ks",21.2,null,"ks",25.863999999999997,"1 ks",25.863999999999997]
["POROTHERM 30  P+D   P-10","ks",31.3,"1 ks",31.3,null,"ks",38.186,"1 ks",38.186]
["POROTHERM 30  P+D  1/2  P-10,15","ks",16.9,"1 ks",16.9,null,"ks",20.618,"1 ks",20.618]
["POROTHERM 24  P+D   P-10","ks",37.8,"1 ks",37.8,null,"ks",46.11599999999999,"1 ks",46.11599999999999]
["POROTHERM 11,5 P+D  P-8/10","ks",32.5,"1 ks",32.5,null,"ks",39.65,"1 ks",39.65]
["POROTHERM 6,5  P+D  P-15","ks",14,"1 ks",14,null,"ks",17.08,"1 ks",17.08]
["KERAMICKÉ PŘEKLADY POROTHERM","ks",null,"1 ks",null,null,"ks",null,"1 ks"]
["SÁDROKARTON"]
["KNAUF GKB   9,5 mm normální","m2",48,"m2",48,null,"m2",58.56,"m2",58.56]
["KNAUF GKB 12,5 mm normální","m2",49,"m2",49,null,"m2",59.78,"m2",59.78]
["KNAUF GKB    15 mm normální","m2",79,"m2",79,null,"m2",96.38,"m2",96.38]
["KNAUF GKB    18 mm normální","m2",97,"m2",97,null,"m2",118.34,"m2",118.34]
["KNAUF GKF 12,5 mm protipožární","m2",71,"m2",71,null,"m2",86.62,"m2",86.62]
["KNAUF GKF   15 mm protipožární","m2",87,"m2",87,null,"m2",106.14,"m2",106.14]
["KNAUF GKF   18 mm protipožární","m2",114,"m2",114,null,"m2",139.07999999999998,"m2",139.07999999999998]
["KNAUF GKB I  12,5 mm vodní","m2",74,"m2",74,null,"m2",90.28,"m2",90.28]
["KNAUF GKB I    15 mm vodní","m2",110,"m2",110,null,"m2",134.2,"m2",134.2]
["KNAUF GKB I  12,5 mm protipožární+vodní","m2",94,"m2",94,null,"m2",114.67999999999999,"m2",114.67999999999999]
["KNAUF GKB I    15 mm protipožární+vodní","m2",110,"m2",110,null,"m2",134.2,"m2",134.2]
["KNAUF profil CW 50","m",19,"m",19,null,"m",23.18,"m",23.18]
["KNAUF profil CW 75","m",22,"m",22,null,"m",26.84,"m",26.84]
["KNAUF profil CW 100","m",25.5,"m",25.5,null,"m",31.11,"m",31.11]
["KNAUF profil CD 60","m",15,"m",15,null,"m",18.3,"m",18.3]
["KNAUF profil UD 30","m",11,"m",11,null,"m",13.42,"m",13.42]
["KNAUF profil UA 50","m",68,"m",68,null,"m",82.96,"m",82.96]
["KNAUF profil UA 75","m",79,"m",79,null,"m",96.38,"m",96.38]
["KNAUF profil UA 100","m",91,"m",91,null,"m",111.02,"m",111.02]
["KNAUF profil UW 50","m",16,"m",16,null,"m",19.52,"m",19.52]
["KNAUF profil UW 75","m",19,"m",19,null,"m",23.18,"m",23.18]
["KNAUF profil UW 100","m",22,"m",22,null,"m",26.84,"m",26.84]
["ŠROUB TN 25","ks",110,"1 ks",110,null,"ks",134.2,"1 ks",134.2]
["ŠROUB TN 35","ks",130,"1 ks",130,null,"ks",158.6,"1 ks",158.6]
["ŠROUB TN 45","ks",130,"1 ks",130,null,"ks",158.6,"1 ks",158.6]
["ŠROUB TN 55","ks",130,"1 ks",130,null,"ks",158.6,"1 ks",158.6]
["TEX šroub LB 9,5/3,5 ","ks",130,"1 ks",130,null,"ks",158.6,"1 ks",158.6]
["UNIFLOT 5kg","ks",140,"1 ks",140,null,"ks",170.79999999999998,"1 ks",170.79999999999998]
["UNIFLOT 25kg","ks",210,"1 ks",210,null,"ks",256.2,"1 ks",256.2]
["LIŠTA  AL / 2m","m",10,"2m",20,null,"m",12.2,"m",24.4]
["ZÁVÉS PŔÍMÝ 60/125mm na CD","ks",3,"1 ks",3,null,"ks",3.66,"1 ks",3.66]
["K - 05 rychlozávěs CD s pérem","ks",4,"1 ks",4,null,"ks",4.88,"1 ks",4.88]
["K - 03 závěs krokvový 125mm","ks",4.1,"1 ks",4.1,null,"ks",5.002,"1 ks",5.002]
["STROPNÍ HŘEB ALU 6/30","ks",2.9,"1 ks",2.9,null,"ks",3.538,"1 ks",3.538]
["VRUT  4,5x40mm","ks",0.55,"1 ks",0.55,null,"ks",0.671,"1 ks",0.671]
["VRUT  4,5x60mm","ks",0.75,"1 ks",0.75,null,"ks",0.915,"1 ks",0.915]
["HMOŽDINKA K-6/35","ks",0.9,"1 ks",0.9,null,"ks",1.098,"1 ks",1.098]
["HMOŽDINKA K-6/55","ks",1.2,"1 ks",1.2,null,"ks",1.464,"1 ks",1.464]
["HMOŽDINKA K-6/60","ks",1.35,"1 ks",1.35,null,"ks",1.647,"1 ks",1.647]
["KNAUF SKELNÁ PÁSKA","ks",23,"1 ks",23,null,"ks",28.06,"1 ks",28.06]
["KNAUF SAMOLEPÍCÍ PÁSKA 45m","ks",77,"1 ks",77,null,"ks",93.94,"1 ks",93.94]
["KNAUF SAMOLEPÍCÍ PÁSKA 90m","ks",147,"1 ks",147,null,"ks",179.34,"1 ks",179.34]
["YTONG"]
["TVÁRNICE 60x25x5","ks",16,"1 ks",16,null,"ks",19.52,"1 ks",19.52]
["TVÁRNICE 60x25x7,5","ks",24,"1 ks",24,null,"ks",29.28,"1 ks",29.28]
["TVÁRNICE 60x25x10","ks",32,"1 ks",32,null,"ks",39.04,"1 ks",39.04]
["TVÁRNICE 60x25x12,5","ks",40,"1 ks",40,null,"ks",48.8,"1 ks",48.8]
["TVÁRNICE 60x25x15","ks",48,"1 ks",48,null,"ks",58.56,"1 ks",58.56]
["TVÁRNICE 60x25x20","ks",58.5,"1 ks",58.5,null,"ks",71.37,"1 ks",71.37]
["TVÁRNICE 60x25x25","ks",73,"1 ks",73,null,"ks",89.06,"1 ks",89.06]
["TVÁRNICE 60x25x30","ks",87,"1 ks",87,null,"ks",106.14,"1 ks",106.14]
["TVÁRNICE 60x25x37,5","ks",109,"1 ks",109,null,"ks",132.98,"1 ks",132.98]
["TVÁRNICE U 50x25x20","ks",102,"1 ks",102,null,"ks",124.44,"1 ks",124.44]
["TVÁRNICE U 50x25x25","ks",125,"1 ks",125,null,"ks",152.5,"1 ks",152.5]
["TVÁRNICE U 50x25x30","ks",147,"1 ks",147,null,"ks",179.34,"1 ks",179.34]
["TVÁRNICE U 50x25x37,5","ks",182,"1 ks",182,null,"ks",222.04,"1 ks",222.04]
["CEMENTOTŘÍSKOVÉ  DESKY"]
["CETRIS  deska 1250 x 3350mm tl.  8 mm","m2",144,"4,19m2",603.36,null,"m2",175.68,"4,19m2",736.0992]
["CETRIS  deska 1250 x 3350mm tl. 10 mm","m2",157.5,"4,19m2",659.9250000000001,null,"m2",192.15,"4,19m2",805.1085]
["CETRIS  deska 1250 x 3350mm tl. 12 mm","m2",172,"4,19m2",720.6800000000001,null,"m2",209.84,"4,19m2",879.2296]
["CETRIS  deska 1250 x 3350mm tl. 14 mm","m2",200,"4,19m2",838.0000000000001,null,"m2",244,"4,19m2",1022.3600000000001]
["CETRIS  deska 1250 x 3350mm tl. 16 mm","m2",231,"4,19m2",967.8900000000001,null,"m2",281.82,"4,19m2",1180.8258]
["CETRIS  deska 1250 x 3350mm tl. 18 mm","m2",259,"4,19m2",1085.21,null,"m2",315.98,"4,19m2",1323.9562]
["CETRIS  deska 1250 x 3350mm tl. 20 mm","m2",288,"4,19m2",1206.72,null,"m2",351.36,"4,19m2",1472.1984]