{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["cenik5"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":32,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"cenik5","index":0,"n_rows":87,"n_cols":10,"rows_kept":87,"cut":false,"hidden":false,"merged":[[1,9,2,9],[0,0,2,0],[48,0,48,9],[3,0,3,9],[36,0,36,9],[0,1,0,4],[0,6,0,9],[1,2,2,2],[1,6,2,6],[1,3,2,3],[1,4,2,4],[1,7,2,7],[1,1,2,1],[1,8,2,8]],"flags":["formulas_cached_only"]}
["název zboží         aktualizováno 3.3.2004","cena  bez DPH",{"$nulls":4},"cena s DPH "]
[null,"měrná     jednotka","za měrnou jednotku","balení","za jedno  balení",null,"měrná     jednotka","za měrnou jednotku","balení","za jedno  balení"]
[]
["TEPELNÉ A ZVUKOVÉ IZOLACE"]
["ROCKWOOL - ROCKMÍN  40mm","m2",39.8,"7,5m2",298.5,null,"m2",48.556,"7,5m2",364.17]
["ROCKWOOL - ROCKMÍN  50mm","m2",49.8,"6 m2",298.79999999999995,null,"m2",60.75599999999999,"6 m2",364.53599999999994]
["ROCKWOOL - ROCKMÍN  60mm","m2",59.8,"5m2",299,null,"m2",72.95599999999999,"5m2",364.78]
["ROCKWOOL - ROCKMÍN  80mm","m2",79.6,"4 m2",318.4,null,"m2",97.112,"4 m2",388.448]
["ROCKWOOL - ROCKMÍN 100mm","m2",99,"3 m2",297,null,"m2",120.78,"3 m2",362.34]
["ROCKWOOL - ROCKMÍN 120mm","m2",119.5,"2,5m2",298.75,null,"m2",145.79,"2,5m2",364.47499999999997]
["ROCKWOOL - ROCKMÍN 140mm","m2",139.4,"2 m2",278.8,null,"m2",170.068,"2 m2",340.136]
["ROCKWOOL - ROCKMÍN 160mm","m2",159.3,"2 m2",318.6,null,"m2",194.346,"2 m2",388.692]
["ROCKWOOL - STEPROCK  T  20mm","m2",55.1,"8 m2",440.8,null,"m2",67.222,"8 m2",537.776]
["ROCKWOOL - STEPROCK  T  30mm","m2",82.7,"6 m2",496.20000000000005,null,"m2",100.894,"6 m2",605.364]
["ROCKWOOL - STEPROCK  T  40mm","m2",110.2,"4 m2",440.8,null,"m2",134.444,"4 m2",537.776]
["ROCKWOOL - STEPROCK  T  50mm","m2",137.8,"3 m2",413.40000000000003,null,"m2",168.116,"3 m2",504.348]
["ORSIL - ORSÍK 40mm","m2",39.7,"6 m2",238.20000000000002,null,"m2",48.434000000000005,"6 m2",290.60400000000004]
["ORSIL - ORSÍK 50mm","m2",49.5,"5 m2",247.5,null,"m2",60.39,"5 m2",301.95]
["ORSIL - ORSÍK 60mm","m2",59.4,"4 m2",237.6,null,"m2",72.468,"4 m2",289.872]
["ORSIL - ORSÍK 80mm","m2",79.2,"3 m2",237.60000000000002,null,"m2",96.624,"3 m2",289.872]
["ORSIL - ORSÍK 100mm","m2",99,"2,5m2",247.5,null,"m2",120.78,"2,5m2",301.95]
["ORSIL - ORSÍK  120mm","m2",118.8,"2 m2",237.6,null,"m2",144.936,"2 m2",289.872]
["ORSIL - ORSÍK  140mm","m2",138.7,"1,5 m2",208.04999999999998,null,"m2",169.21399999999997,"1,5 m2",253.82099999999997]
["ORSIL - ORSÍK  160mm","m2",158.4,"1,5 m2",237.60000000000002,null,"m2",193.248,"1,5 m2",289.872]
["ORSIL - ORSTROP 40mm","m2",38.5,"6 m2",231,null,"m2",46.97,"6 m2",281.82]
["ORSIL - ORSTROP 50mm","m2",48.2,"5 m2",241,null,"m2",58.804,"5 m2",294.02]
["ORSIL - ORSTROP 60mm","m2",57.7,"4 m2",230.8,null,"m2",70.394,"4 m2",281.576]
["ORSIL - ORSTROP 80mm","m2",76.9,"3 m2",230.70000000000002,null,"m2",93.818,"3 m2",281.454]
["ORSIL - ORSTROP 100mm","m2",96.1,"2,5m2",240.25,null,"m2",117.24199999999999,"2,5m2",293.105]
["ORSIL - ORSTROP  120mm","m2",115.5,"2 m2",231,null,"m2",140.91,"2 m2",281.82]
["ORSIL - ORSTROP  140mm","m2",134.7,"1,5 m2",202.04999999999998,null,"m2",164.33399999999997,"1,5 m2",246.50099999999998]
["ORSIL - ORSTROP  160mm","m2",154,"1,5 m2",231,null,"m2",187.88,"1,5 m2",281.82]
["ORSIL  N 20 mm","m2",55.1,"12 m2",661.2,null,"m2",67.222,"12 m2",806.664]
["ORSIL  N 25 mm","m2",69,"9 m2",621,null,"m2",84.17999999999999,"9 m2",757.62]
["ORSIL  N 40 mm","m2",110,"6 m2",660,null,"m2",134.2,"6 m2",805.1999999999999]
["ORSIL  N 50 mm","m2",137.6,"4 m2",550.4,null,"m2",167.87199999999999,"4 m2",671.4879999999999]
["FÓLIE"]
["fólie PE 0,1x800 mm polorukáv - 40m2","ks",470,"1 ks",470,null,"ks",573.4,"1 ks",573.4]
["fólie PE 0,1x1000 mm","kg",63,"1 kg",63,null,"kg",76.86,"1 kg",76.86]
["fólie PE 0,1x1200 mm","kg",63,"1 kg",63,null,"kg",76.86,"1 kg",76.86]
["fólie Jutafol D 75 m2 paropropustná","m2",15.5,"75 m2",1162.5,null,"m2",18.91,"75 m2",1418.25]
["fólie Jutafol N 75 m2 parotěsná","m2",15.5,"75 m2",1162.5,null,"m2",18.91,"75 m2",1418.25]
["fólie Parofol AL 1,2/100m parotěsná","m2",25,"120 m2",3000,null,"m2",30.5,"120 m2",3660]
["GEOTEXTILIE  150 g / m2 ","m2",15.9,"100 m2",1590,null,"m2",19.398,"100 m2",1939.8]
["GEOTEXTILIE  200 g / m2 ","m2",18.9,"100 m2",1889.9999999999998,null,"m2",23.057999999999996,"100 m2",2305.7999999999997]
["GEOTEXTILIE  300 g / m2 ","m2",24.9,"100 m2",2490,null,"m2",30.377999999999997,"100 m2",3037.7999999999997]
["PERLINKA  SAKRET","m2",29,"1 m2",29,null,"m2",35.38,"1 m2",35.38]
["PERLINKA","m2",26,"1 m2",26,null,"m2",31.72,"1 m2",31.72]
["POLYSTYRÉN"]
[" PSB - S - 20kg samozhášivý 10 mm","m2",15,"25m2",375,null,"m2",18.3,"25m2",457.5]
[" PSB - S - 20kg samozhášivý 20 mm","m2",25,"12,5m2",312.5,null,"m2",30.5,"12,5m2",381.25]
[" PSB - S - 20kg samozhášivý 30 mm","m2",38,"8 m2",304,null,"m2",46.36,"8 m2",370.88]
[" PSB - S - 20kg samozhášivý 40 mm","m2",50,"6 m2",300,null,"m2",61,"6 m2",366]
[" PSB - S - 20kg samozhášivý 50 mm","m2",63,"5 m2",315,null,"m2",76.86,"5 m2",384.3]
[" PSB - S - 20kg samozhášivý 60 mm","m2",75," 4 m2",300,null,"m2",91.5," 4 m2",366]
[" PSB - S - 20kg samozhášivý 80 mm","m2",100,"3 m2",300,null,"m2",122,"3 m2",366]
[" PSB - S - 20kg samozhášivý 100 mm","m2",125,"2,5m2",312.5,null,"m2",152.5,"2,5m2",381.25]
[" PSB - S - 20kg samozhášivý 120 mm","m2",150,"2m2",300,null,"m2",183,"2m2",366]
[" PSB - S - 25kg samozhášivý 10 mm","m2",15,"25m2",375,null,"m2",18.3,"25m2",457.5]
[" PSB - S - 25kg samozhášivý 20 mm","m2",29,"12,5m2",362.5,null,"m2",35.38,"12,5m2",442.25]
[" PSB - S - 25kg samozhášivý 30 mm","m2",44,"8 m2",352,null,"m2",53.68,"8 m2",429.44]
[" PSB - S - 25kg samozhášivý 40 mm","m2",58,"6 m2",348,null,"m2",70.76,"6 m2",424.56]
[" PSB - S - 25kg samozhášivý 50 mm","m2",73,"5 m2",365,null,"m2",89.06,"5 m2",445.3]
[" PSB - S - 25kg samozhášivý 60 mm","m2",87," 4 m2",348,null,"m2",106.14," 4 m2",424.56]
[" PSB - S - 25kg samozhášivý 80 mm","m2",116,"3 m2",348,null,"m2",141.52,"3 m2",424.56]
[" PSB - S - 25kg samozhášivý 100 mm","m2",145,"2,5m2",362.5,null,"m2",176.9,"2,5m2",442.25]
[" PSB - S - 25kg samozhášivý 120 mm","m2",174,"2m2",348,null,"m2",212.28,"2m2",424.56]
[" PSB - S - 20kg stabil fasádní 10 mm","m2",13,"25m2",325,null,"m2",15.86,"25m2",396.5]
[" PSB - S - 20kg stabil fasádní 20 mm","m2",26,"12,5m2",325,null,"m2",31.72,"12,5m2",396.5]
[" PSB - S - 20kg stabil fasádní 30 mm","m2",39,"8 m2",312,null,"m2",47.58,"8 m2",380.64]
[" PSB - S - 20kg stabil fasádní 40 mm","m2",52,"6 m2",312,null,"m2",63.44,"6 m2",380.64]
[" PSB - S - 20kg stabil fasádní 50 mm","m2",65,"5 m2",325,null,"m2",79.3,"5 m2",396.5]
[" PSB - S - 20kg stabil fasádní 60 mm","m2",78," 4 m2",312,null,"m2",95.16," 4 m2",380.64]
[" PSB - S - 20kg stabil fasádní 80 mm","m2",104,"3 m2",312,null,"m2",126.88,"3 m2",380.64]
[" PSB - S - 20kg stabil fasádní 100 mm","m2",113,"2,5m2",282.5,null,"m2",137.85999999999999,"2,5m2",344.65]
[" PSB - S - 20kg stabil fasádní 120 mm","m2",156,"2m2",312,null,"m2",190.32,"2m2",380.64]
["extrudovaný Glacsofoam XPS -III 20 mm","m2",92,"15 m2",1380,null,"m2",112.24,"15 m2",1683.6]
["extrudovaný Glacsofoam XPS -III 30 mm","m2",138,"9,75m2",1345.5,null,"m2",168.35999999999999,"9,75m2",1641.51]
["extrudovaný Glacsofoam XPS -III 40 mm","m2",184,"7,5m2",1380,null,"m2",224.48,"7,5m2",1683.6]
["extrudovaný Glacsofoam XPS -III 50 mm","m2",230,"6 m2",1380,null,"m2",280.59999999999997,"6 m2",1683.6]
["extrudovaný Glacsofoam XPS -III 60 mm","m2",276,"4,5 m2",1242,null,"m2",336.71999999999997,"4,5 m2",1515.24]
["extrudovaný Glacsofoam XPS -III 80 mm","m2",368,"3,75m2",1380,null,"m2",448.96,"3,75m2",1683.6]
["extrudovaný Glacsofoam XPS -III 100 mm","m2",460,"3 m2",1380,null,"m2",561.1999999999999,"3 m2",1683.6]
["LIGNOPOR 2,5cm","m2",113,"1 m2",113,null,"m2",137.85999999999999,"1 m2",137.85999999999999]
["LIGNOPOR 3,5cm","m2",132,"1 m2",132,null,"m2",161.04,"1 m2",161.04]
["LIGNOPOR 5cm","m2",170,"1 m2",170,null,"m2",207.4,"1 m2",207.4]
["LIGNOPOR 7,5cm","m2",222,"1 m2",222,null,"m2",270.84,"1 m2",270.84]